TSE X50
Public beta / Development version 13.04.2011

This plugin is still in development, it's previewed to get people's opinions and tips/feedback regarding improvement of sound/nitpicks..
The plugin is at this stage pretty heavy on the CPU compared to most ampsims on the market today, so you've been warned. Mix at low quality settings and enable high quality before mixdown.. or just freeze/bounce etc if it becomes a pain in the ass.

The green channel is to be revisited before final release, it's a bit off ;)

The poweramp has a selectable tubes/adjustable bias etc.. If you change a tube, you also need to change the bias and search for that particular "sweet spot" according to your taste.
Each tube has different gain, so you might have to compensate for volume with the output control as no normalization is implemented. The 6L6GC and EL34 tubes has recommended bias settings as of -51V and -39V,
use your ears :P 
Also found in the poweramp section is the negative feedback, there are two settings/models on that circuit. A "dynamic" which is determined by the overall gain of the phasesplitter/poweramp as it appears in
this model, or a "static" which is calibrated after reamps of the actual amp. The difference is barely noticable.


Have fun helping me improve this thing!


- John Adrian Johansen

/onQel



Changes in B3:

- Volume control goes louder.
- Disabled bright/crunch switches on Red channel
- Disabled Red.Ch Mod switch on Green channel
- Updated contitions for tubeswitching, to prevent clicks/glitches when a control is changed
- Changed the way to calculate miller capacitances.  Result is less noise etc.
- Changed a bad capacitor value in NFB-loop. HIFI-switch introduced to keep the B2 sound.
- Tweaked the resonance control to behave better.
- Edited small buttons for visibility
- Tweaks in the gainstage-model in an attempt to save cpu.